140/01 DUCT/ WALL LININGS – WITH FRAMES

* Drawing reference(s): D.MDF.LH, D.MDF.SH, D.MDF.EH
* Manufacturer and reference: Aaztec Associates Ltd. (Aaztec Washrooms) Becklands Close, Bar Lane, Boroughbridge, N.Yorks, YO51 9NR.

Tel: 01423 326400 Email: sales@aaztec.com

* Product: **SGL/CDF Ducts – MDF Frames**

Design/Height: See options below.

Panels:

* Material/Thickness: 12-13mm nominal Solid Grade laminate (SGL) or 12-13mm nominal Compact Density Fibre Board (CDF) finished with choice of laminate colour.
* Edge treatment: Half bull nose to all edges.
* Colour/Finish: From our standard range.

Flash Gaps:

* Material/Thickness: 12-13mm nominal Solid Grade laminate (SGL) or 12-13mm nominal Compact Density Fibre Board (CDF) finished with choice of laminate colour.
* Edge treatment: No treatment (Saw cut).
* Colour/Finish: From our standard range.

Supporting framework:

* Material/Thickness: Constructed from 18mm Medium Density Fibreboard (MDF)
* Method of fixing: Concealed plastic keku clips fitted to internal sections of the frames and reverse of access panels. Counter sink screws to flashing strips and timber fixing rails. The number of wall batons used are at the installer’s discretion.
* Joint treatment: Nominal 50mm wide flashgap between each panel section or too partition face and 100mm high plinth and header flashgap. Flashgaps can be adjusted.
* Fixings: keku clips with screws and drill bit supplied
* Included features: Lift-off access panels fitted with plastic keku clips.
* Assembly: Access panels pre-fitted to framework. Flashing strips supplied loose with no holes pre-drilled to scribe on site. Optional top lid and end return are supplied oversized to scribe on site. Timber top and bottom rails and wall batons are required.

Height options (see diagrams)

Low height (1200-2000mm)

Full height (2000-2600mm)

Extended height (Over 2600mm) (Split top panel with 30mm flash gap between)

Panel split options (see diagrams)

Back to wall pan

Wall hung pan

Urinal

Sink with exposed trap and waste

Sink with concealed trap and waste

Optional extras

Header to be extended above the ceiling line by 50mm

Push-on keku clips

End return

Side hinged & lockable access panel

Top hinged & lockable access panel

Top hinged & push to lock access panel

DDA compliant panel and flashing splits